TABLE 4-9. NAVY TEEN/STAFF/VISITOR TOILETS

|  |  |
| --- | --- |
| **Description/ Usage** | Navy provides multiple (as needed) unisex toilets for use by Teens, Staff and visitors. Quantity of toilets is based on the applicable code for the calculated occupancy. The other Services do not use unisex toilets. See Table 3-1 for Service-specific toilet requirements. |
| **Min. Ceiling Ht.** | 2.44 m (8 ft.) minimum. |
| **Finishes** | **Walls.**  Epoxy or enamel painted, moisture-resistant gypsum wallboard with a ceramic tile wainscot. Provide full-height ceramic tile on wet walls; consider full-height ceramic tile on all walls. |
|  | **Floor.** Ceramic tile. |
|  | **Ceiling.** Painted, moisture-resistant gypsum board. |
| **Plumbing** | One wall-hung water closet and lavatory. Provide a floor drain. |
| **HVAC** | 20 C (68 F) minimum, 26 C (78 F) maximum. Ventilate to the exterior per code. |
| **Fire Protection** | Provide system per paragraph 3-5.3. |
| **Power** | Provide outlets per code. |
| **Lighting** | 540 lux (50 fc). |
| **Communication** | **CCTV.** None required.  **CATV/Internal Video.** None required.  **PA/Audio.** None required.  **Telephone.** None required.  **Data.**  None required.  **Security.** Lockable door. |
| **Casework** | Solid-surface countertop supported at both ends with either underhung or integral sink. A wall-hung lavatory is also acceptable.  Wall-hung water closets. |
| **Furnishings Fixtures & Equipment (FF&E)** | Toilet accessories: toilet paper dispensers, paper towel dispenser with integrated trash receptacle, robe hooks, grab bars, and soap dispensers.  Mirror. |
| **Special Requirements** | This room must be ADA-compliant. |
| For use during project execution by the appropriate Service agency | |
| **Occupancy** | Staff. |
|  | Patrons/Youth. |
| **Min. net m2 (ft2)** |  |