TABLE 4-4.1. SAC ACTIVITY ROOMS

|  |  |
| --- | --- |
| **Description/ Usage** | These rooms accommodate a variety of activities and program options for youth in the SAC program. These rooms may be used for multiple activities such as arts/crafts, hobbies, performing arts/drama, science, and study. The room should be able to accommodate multiple activities at the same time.  Note: the Services vary on how they configure these rooms; see floor finishes below for more information. |
| **Min. Ceiling Ht.** | 2.44 m (8 ft.) minimum and (12 ft.) maximum. |
| **Finishes** | **Walls.**  Gypsum wallboard—first 1.22 m (4 ft.) with a protective wall covering wainscot and paint above 1.22 m (4 ft.). |
|  | **Floor.** Provide 100% hard surface flooring (prefer vinyl composition tile) and the use of area carpets to allow flexibility of room configuration. Vinyl or rubber base.  Air Force requires 50% carpet (in clean area), 50% seamless, impervious, non-skid, non-textured hard-surface flooring (in play area). Vinyl or rubber base.  Navy will allow stained concrete for hard-surface flooring. |
|  | **Ceiling.** ACP. |
| **Plumbing** | Provide one two-compartment sink with hot and cold water. To facilitate arts and crafts activities, consider making this a deep sink. To prevent scalding of youth, limit water temperature to 43 C (110 F). Provide a floor drain. |
| **HVAC** | 20 C (68 F) minimum, 26 C (78 F) maximum. |
| **Fire Protection** | Provide system per paragraph 3-5.3. |
| **Power** | Provide duplex outlets at 2.44 m (8 ft.) on center at perimeter walls; provide at least one GFI duplex above countertop; provide duplex outlets for TV (near cable outlet), refrigerator, and microwave. |
| **Lighting** | 540 lux (50 fc) minimum. Consider providing as much as 750 lux (70 fc) to accommodate arts and craft activities. |
| **Communication** (in each room) | **CCTV.**  Provide minimum one outlet. Consider the shape of the room and the panning range of the camera to determine if additional outlets will be necessary.  **CATV/Internal Video.** Provide one outlet.  Navy does not support CATV in this space.  **PA/Audio.**  Provide a speaker.  **Telephone.** Provide one line with internal two-way communication.  **Data.**  Consider providing at least two outlets.  **Security.** Do not create corners or “nooks” not visible from other areas of the room. |
| **Casework** | Provide lockable base and wall cabinets with adjustable shelves. Solid surface countertops are required where water is present and preferred elsewhere. |
| **Furnishings Fixtures & Equip. (FF&E)** | Tables, chairs, soft seating areas, computers, tack board, and marker board. Consider age-appropriate dimensions for all furniture and fixtures.  Consider providing undercounter refrigerator and microwave for life skills training.  Provide storage for each youth. Consider individual lockers. |
| **Special Requirements** | Provide tackable surfaces on the walls.  Include vision panels in interior doors and large windows in the interior walls. Provide exterior doors to outside activity area.  Army requires exterior doors to be alarmed. Navy does not require exterior doors.  Provide a dedicated storage closet (the space for this has been included in the space program) with hanging rods and/or shelves for each SAC Activity Room. |
| For use during project execution by the appropriate Service agency | |
| **Occupancy** | Staff. |
|  | Patrons/Youth. |
| **Min. net m2 (ft2)** | Room. Storage Closet. |